
**HYL-030DA0700G097AD\_DALI 2**

Constant current LED driver

DALI Dimmable

**Product description**

* Dimmable Independent constant current LED Driver
* Adjustable output current between350 and 700mA

via DIP switch, Factory default setting 350mA gear

* Max. output power 30W
* Up to 85 % efficiency
* Power input on stand-by < 0.3 W
* Dimming range 1 – 100 %
* For luminaires of protection class I and protection class II
* Nominal life-time up to 50,000 h
* 5-year guarantee

**Benefits**

* Application-oriented operating window for maximum compatibility
* Best energy savings due to low stand-by losses and high efficiency
* Long lasting and high reliability
* Classic compact housing

**Interfaces**

* DALI （DT-6）
* SwitchDIM\PUSH DIM (with memory function)
* Terminal blocks: 45° push terminals



**Applications**

* Linear and area lighting
* Office – industrial – shop



**Approval marks**



In preparation, if not already printed on product label

**Technical data**

****

Units：mm

ON

OFF

●

○

DIP Switch

DIP Switch

ON

OFF

**Ordering data**



**Specific technical data**

****

①Load switching on output side is safe but not permitted

②Valid at 100 % dimming level

|  |  |
| --- | --- |
| **ACCES­SORIES** |  |

**Product description**

* Optional strain-relief set for independent applications
* Transforms the LED Driver into a fully class II compatible LED Driver

(e.g. ceiling installation)





Figure 2

Figure 1

**Ordering data**

